InstitutoImagen que contiene dibujo, alimentos

Descripción generada automáticamenteIcono

Descripción generada automáticamente

Politécnico

Nacional

Escuela Superior de Cómputo

**Practica 2.3. VLAN**

Materia:

Administración de servicios en red

Grupo:

4CV13

Profesor:

Henestrosa Carrasco Leticia

Integrantes: (***Equipo 1***)

Arévalo Andrade Miguel Ángel

Castro Cruces Jorge Eduardo

López Mares Irene Elizabeth

Pedroza García Rodolfo

Fecha:

jueves, 31 de marzo de 2022

**Activity 2.3.8:  
Configuring Basic Switch Management**

**NOTE TO USER:** Although you can complete this activity without printed instructions, a PDF version is available on the text side of the same page from which you launched this activity.

**Addressing Table**

| **Device** | **Interface** | **IP Address** | **Subnet Mask** |
| --- | --- | --- | --- |
| **S1** | **VLAN99** | 172.17.99.11 | 255.255.255.0 |
| **PC1** | **NIC** | 172.17.99.21 | 255.255.255.0 |
| **Server** | **NIC** | 172.17.99.31 | 255.255.255.0 |

**Learning Objectives**

* Connect to the switch using a console connection
* Navigate through various CLI modes
* Use the Help Facility to configure the clock
* Access and configure command history
* Configure the boot sequence
* Configure a PC and connect it to a switch
* Configure full duplex
* Manage the MAC address table
* Manage the switch configuration file

**Introduction:**

Basic switch management is the foundation for configuring switches. This activity focuses on navigating command-line interface modes, using help functions, accessing the command history, configuring boot sequence parameters, setting speed and duplex settings, as well as managing the MAC address table and switch configuration file. Skills learned in this activity are necessary for configuring basic switch security in later chapters.

**Task 1: Connect to the Switch**

**Step 1. Connect S1 and PC1.**

* Using a console cable, connect the RS 232 interface on PC1 to the console interface on switch S1.
* Click **PC1** and then click the **Desktop** tab. Select **Terminal** in the Desktop tab.
* Keep these default settings for Terminal Configuration and then click **OK**:
  + Bits Per Second = 9600
  + Data Bits = 8
  + Parity = None
  + Stop Bits = 1
  + Flow Control = None
* You are now consoled into S1. Press **Enter** to get the Switch prompt.

**Step 2. Check results.**

Your completion percentage should be 6%. If not, click Check Results to see which required components are not yet completed.

**Task 2: Navigate Through CLI Modes**

**Step 1. In user EXEC mode, type ?. Note the list of available commands.**

While in user EXEC mode, the available commands are limited to basic monitoring commands.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 2. Use the enable command to go to privileged EXEC mode.**

Switch>**enable**

Switch#

The prompt changes from > to #.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 3. In privileged EXEC mode, type ?. Note the list of available commands.**

There are now more available commands compared to user EXEC mode. In addition to the basic monitoring commands, configuration and management commands can now be accessed.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 4. Change to global configuration mode.**

Switch#**configure terminal**

Switch(config)#

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 5. In global configuration mode, type ?. Note the list of available commands.**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 6. Configure S1 as the hostname.**

Switch(config)#**hostname S1**

S1(config)#

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 7. Change to interface configuration mode for VLAN99.**

The **interface vlan 99** command creates the interface and changes to interface configuration mode for VLAN99.

S1(config)#**interface vlan 99**

S1(config-if)#

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 8. Configure VLAN99 with 172.17.99.11/24 and activate the interface.**

Use the **ip address** and **no shutdown** commands to assign the correct IP address/subnet mask and activate the interface.

S1(config-if)#**ip address 172.17.99.11 255.255.255.0**

S1(config-if)#**no shutdown**

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 9. Change to interface configuration mode for Fa0/18.**

S1(config-if)#**interface fa0/18**

S1(config-if)#

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 10. Set the port mode to access.**

To allow for frames to be sent and received from the interface, change the switching mode to access using the **switchport mode access** command.

S1(config-if)#**switchport mode access**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 11. Assign VLAN99 to the port.**

To allow the Fa0/18 interface to act as a member of VLAN 99, issue the **switchport access vlan 99** command.

S1(config-if)#**switchport access vlan 99**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 12. Exit interface configuration mode.**

Issue the **exit** command to leave interface configuration mode and enter global configuration mode.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Step 13. Enter configuration mode for the console line.**

S1(config)#**line console 0**

S1(config-line)#

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 14. In line configuration mode, type ?. Note the list of available commands.**

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 15. Enter cisco as the password.**

S1(config-line)#**password cisco**

S1(config-line)#**login**

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 16. Return to privileged EXEC mode using the end command.**

S1(config-line)#**end**

S1#

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 17. Check results.**

Your completion percentage should be 31%. If not, click **Check Results** to see which required components are not yet completed.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 3: Use Help Facility to Configure the Clock**

**Step 1. At the privileged EXEC command prompt, type clock ?.**

S1#**clock ?**

The only option is **set**.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 2. Use Help to assist setting the clock to the current time.**

S1#**clock ?**

set Set the time and date

S1#**clock set ?**

hh:mm:ss Current Time

S1#**clock set 12:12:12 ?**

<1-31> Day of the month

MONTH Month of the year

Continue issuing the **?** command until you have completed configuring the clock. You are warned with a % **Incomplete command message** if the **clock** command is not fully entered with all the required arguments.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 3. Verify that the clock is set.**

To verify that the clock is set, issue the **show clock** command. **Note:** Packet Tracer does not always show the correct time configured. Completion is still at 31% at the end of this Task.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 4: Access and Configure Command History**

**Step 1. View the most recent commands entered.**

Issue the **show history** command. Remember how many commands are listed.

S1#**show history**

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 2. Change the number of commands stored in the history buffer.**

Enter line configuration mode for both the console and Telnet lines. Set the number of commands held in the history buffer to 35.

S1(config)#**line console 0**

S1(config-line)#**history size 35**

S1(config-line)#**line vty 0 4**

S1(config-line)#**history size 35**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 3. Verify that the size of the history buffer has changed.**

Return to privileged EXEC mode and issue the **show history** command again. There should be more commands displayed than previously.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 4. Check results.**

Your completion percentage should be 50%. If not, click **Check Results** to see which required components are not yet completed.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 5: Configure the Boot Sequence**

**Step 1. Check which Cisco IOS software version is currently loaded.**

S1#**show version**

Cisco IOS Software, C2960 Software (C2960-LANBASE-M), Version 12.2(25)FX, RELEASE SOFTWARE (fc1)

Copyright (c) 1986-2005 by Cisco Systems, Inc.

Compiled Wed 12-Oct-05 22:05 by pt\_team

<output omitted>

The version is listed in the first line.

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 2. Check which Cisco IOS images are loaded in flash memory.**

S1#**show flash**

Directory of flash:/

3 -rw- 4414921 c2960-lanbase-mz.122-25.FX.bin

2 -rw- 4670455 c2960-lanbase-mz.122-25.SEE1.bin

6 -rw- 616 vlan.dat

32514048 bytes total (23428056 bytes free)

Note that there are two versions in flash memory. The version that is currently loaded is **c2960-lanbase-mz.122-25.FX.bin.**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 3. Configure the system to boot using a different Cisco IOS image.**

In global configuration mode, issue this command.

S1(config)#**boot system flash:/c2960-lanbase-mz.122-25.SEE1.bin**

**Note:** Although you can enter this command in Packet Tracer, the switch still loads the first image listed in flash.

Una captura de pantalla de una computadora

Descripción generada automáticamente

Packet Tracer does not grade the **boot system** command on switches, so completion remains at 50% at the end of this task.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 6: Configure a PC and Connect it to a Switch**

**Step 1. Configure PC1 with the IP address/subnet mask 172.17.99.21/24.**

* Exit the terminal to return to the **Desktop**tab.
* Click **IP Configuration** and set the IP address to 172.17.99.21 and subnet mask to 255.255.255.0

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 2. Connect PC1 to Fa0/18 on the switch.**

Using the copper straight-through cable, connect the FastEthernet port of the PC to the Fa0/18 port on the switch.

Texto, Word

Descripción generada automáticamente

**Step 3. Test connectivity between S1 and PC1.**

Ping between S1 and PC1. It may take a few attempts, but it should be successful.

Texto, Word

Descripción generada automáticamente

**Step 4. Check results.**

Your completion percentage should be 69%. If not, click **Check Results** to see which required components are not yet completed.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 7: Configure Duplex and Speed**

**Step 1. Use the Config tab change the settings.**

On PC1, select the **Config** tab. Set the bandwidth of the FastEthernet interface to 100 Mbps and Full Duplex.

Interfaz de usuario gráfica, Aplicación

Descripción generada automáticamente

**Step 2. Use Cisco IOS commands to set Fa0/18.**

Return to the desktop and select **Terminal**, and then configure the interface.

S1(config)#**interface fa0/18**

S1(config-if)#**duplex full**

S1(config-if)#**speed 100**

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 3. Test connectivity between S1 and PC1.**

Issue a ping from S1 to PC1. It may take a few attempts, but it should be successful.

Texto, Word

Descripción generada automáticamente

**Step 4. Check results.**

Your completion percentage should be 81%. If not, click **Check Results** to see which required components are not yet completed.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 8: Manage the MAC Address Table**

**Step 1. Check the MAC address of the server.**

Click the **Server**, then the **Config** tab, and then **FastEthernet**. The MAC Address is 0060.3EDD.19A3.

**Step 2. Configure static MAC for the TFTP server.**

By configuring a static MAC for the TFTP server, the switch always knows which port to use to send out traffic destined for the server. In global configuration mode on S1, add the MAC address to the addressing table of the switch:

S1(config)#**mac-address-table static 0060.3EDD.19A3 vlan 99 int fa0/24**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 3. Verify that the static MAC address is now in the MAC address table.**

S1#**show mac-address-table**

Mac Address Table

-------------------------------------------

Vlan Mac Address Type Ports

---- ----------- -------- -----

99 0060.3edd.19a3 STATIC Fa0/24

99 0060.5c5b.cd23 DYNAMIC Fa0/18

S1#

Una captura de pantalla de una computadora

Descripción generada automáticamente

Notice how the MAC address from PC1 was added dynamically. This entry may or may not be in your table depending on how long it has been since you pinged from PC1 to S1.

**Step 4. Test connectivity between S1 and PC1.**

Issue a ping from S1 to PC1. It may take a few attempts, but the command should be successful.

Texto, Word

Descripción generada automáticamente

Packet Tracer does not grade this command. This command is needed to allow the switch to know where to send traffic destined for the server. Completion is still at 81% at the end of this task.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Task 9: Manage the Switch Configuration File**

Using a copper straight-through cable, connect the FastEthernet port on the server to the Fa0/24 port on the switch.

Texto, Word

Descripción generada automáticamente

**Step 1. Enter interface configuration mode for Fa0/24.**

S1#**configure terminal**

S1(config)#**interface fa0/24**

S1(config-if)#

Interfaz de usuario gráfica, Texto

Descripción generada automáticamente

**Step 2. Set the port mode to access.**

Setting the port mode to access allows frames to be sent and received from the interface.

S1(config-if)#**switchport mode access**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 3. Assign VLAN99 to the port.**

Assigning VLAN99 to the port allows the Fa0/24 interface to act as a member of VLAN 99.

S1(config-if)#**switchport access vlan 99**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 4. Verify S1 can ping the server.**

Ping the server from S1. It may take a few attempts, but it should be successful.

Texto, Word

Descripción generada automáticamente

**Step 5. Back up the startup configuration to the server.**

In privileged EXEC mode, copy the startup configuration to the sever. When you are prompted for the address of the remote host, enter IP address of the server, 172.17.99.31. For the destination filename, use the default filename by pressing **Enter**.

S1#**copy startup-config tftp:**

Address or name of remote host []? **172.17.99.31**

Destination filename [S1-confg]? **[Enter]**

Una captura de pantalla de una computadora

Descripción generada automáticamente

**Step 6. Verify that the server has the startup configuration.**

To determine if the startup configuration was successfully transferred to the server, click the server and then click the **Config** tab. The S1-confg file should be listed under Services and TFTP. **Note:** Restoring the startup from the server is not fully simulated in Packet Tracer.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Step 7. Check results.**

Your completion percentage should be 100%. If not, click **Check Results** to see which required components are not yet completed.

Interfaz de usuario gráfica, Texto, Aplicación

Descripción generada automáticamente

**Conclusiones:**

**Arévalo Andrade Miguel Ángel:**

Se cumplieron los objetivos:

• Conéctese al conmutador mediante una conexión de consola

• Navegar a través de varios modos CLI

• Use la función de ayuda para configurar el reloj

• Acceder y configurar el historial de comandos

• Configurar la secuencia de arranque

• Configurar una PC y conectarla a un switch

• Configurar dúplex completo

• Administrar la tabla de direcciones MAC

• Administrar el archivo de configuración del switch

**Castro Cruces Jorge Eduardo:**

Se cumplieron los objetivos principales de la práctica:

* Connect to the switch using a console connection
* Navigate through various CLI modes
* Use the Help Facility to configure the clock
* Access and configure command history

**López Mares Irene Elizabeth:**

Está práctica nos ayudo a observar mejor el funcionamiento de las vlan ya que pudimos crear una red lógica dentro de la red física, además también pudimos manejar diferentes comandos dentro del switch por primera vez, como fueron cambiarle el nombre, configurar el reloj, configurar duplex entre otros.

**Pedroza García Rodolfo:**

En esta práctica interactuamos con el switch, a través de diferentes modos de consola, configuramos una vlan básica, también se configuro direcciones MAC, y además aprendimos a configurar el reloj del switch. Fue una practica introductoria a los switches y aprendimos configuraciones básicas de estos.